OEM Bit disabled (default)


System Bootstrap, Version 12.4(13r)T, RELEASE SOFTWARE (fc1)
Technical Support: http://www.cisco.com/techsupport
Copyright (c) 2006 by cisco Systems, Inc.

Initializing memory for ECC
.
c2811 platform with 262144 Kbytes of main memory
Main memory is configured to 64 bit mode with ECC enabled


Readonly ROMMON initialized
program load complete, entry point: 0x8000f000, size: 0xcb80
program load complete, entry point: 0x8000f000, size: 0xcb80

program load complete, entry point: 0x8000f000, size: 0x416a574
Self decompressing the image : ######################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################## [OK]

Smart Init is enabled
smart init is sizing iomem
  ID            MEMORY_REQ                 TYPE
0003E7          0X00474800 C2811 Mainboard
000024          0X00019A40 Four port Async/Sync
000056          0X000C2800 4-port FE Switch HWIC
                0X00264050 Onboard VPN
                0X000021B8 Onboard USB
                0X002C29F0 public buffer pools
                0X00211000 public particle pools
-----------------------------------------------
TOTAL:          0X00C8A638

If any of the above Memory Requirements are 
"UNKNOWN", you may be using an unsupported
configuration or there is a software problem and
system operation may be compromised.
Rounded IOMEM up to: 14Mb.
Using 5 percent iomem. [14Mb/256Mb]

********************
********************

              Restricted Rights Legend

Use, duplication, or disclosure by the Government is
subject to restrictions as set forth in subparagraph
(c) of the Commercial Computer Software - Restricted
Rights clause at FAR sec. 52.227-19 and subparagraph
(c) (1) (ii) of the Rights in Technical Data and Computer
Software clause at DFARS sec. 252.227-7013.

           cisco Systems, Inc.
           170 West Tasman Drive
           San Jose, California 95134-1706

********************
********************

Cisco IOS Software, 2800 Software (C2800NM-ADVENTERPRISEK9-M), Version 15.3(3)XB12, RELEASE SOFTWARE (fc2)
Technical Support: http://www.cisco.com/techsupport
Copyright (c) 1986-2013 by Cisco Systems, Inc.
Compiled Tue 19-Nov-13 02:16 by prod_rel_team


This product contains cryptographic features and is subject to United
States and local country laws governing import, export, transfer and
use. Delivery of Cisco cryptographic products does not imply
third-party authority to import, export, distribute or use encryption.
Importers, exporters, distributors and users are responsible for
compliance with U.S. and local country laws. By using this product you
agree to comply with applicable laws and regulations. If you are unable
to comply with U.S. and local laws, return this product immediately.

A summary of U.S. laws governing Cisco cryptographic products may be found at:
http://www.cisco.com/wwl/export/crypto/tool/stqrg.html

If you require further assistance please contact us by sending email to
export@cisco.com.

Installed image archive
Cisco 2811 (revision 1.0) with 247808K/14336K bytes of memory.
Processor board ID FTX1214A3DM
6 FastEthernet interfaces
4 Low-speed serial(sync/async) interfaces
1 Virtual Private Network (VPN) Module
DRAM configuration is 64 bits wide with parity enabled.
239K bytes of non-volatile configuration memory.
250880K bytes of ATA CompactFlash (Read/Write)



Press RETURN to get started!

